; 
; ITERAID.INF
; 
; INF file of IT8212 ATA RAID controller for Windows 2000/XP
; Copyright (c) 2002-2004 Integrated Technology Express, Inc. All rights reserved
;

[Version]
Signature="$Windows NT$"
Provider=%ITE%
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
CatalogFile=iteraid.cat
DriverVer=06/01/2004,1.7.1.9

[DestinationDirs]
DefaultDestDir = 12             ; DIRID_DRIVERS (this is IOSubsys on
                                ; Win95, and System32\Drivers on NT)

;
; Driver information
;

[Manufacturer]
%ITE%   = ITE.Mfg

[ITE.Mfg]
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_00011283	; 8212/CX
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_00000000	; 8212/DX
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8211&SUBSYS_82111283	; 8211/DX
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_2A1D103C	; ASUS OEM
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8211&SUBSYS_2A1D103C	; ASUS OEM
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_813A1043	; ASUS 8212
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_81381043	; ASUS 8211
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8211&SUBSYS_81381043	; ASUS 8211
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_2C0717F2	; Albatron 8212
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_1458B000	; Gigabyte 8212
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_1940B000	; Gigabyte 8212
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8212&SUBSYS_0A46174B	; 8212/DX
%ITE.DeviceDesc0% = iteraid, PCI\VEN_1283&DEV_8211&SUBSYS_0A46174B	; 8211/DX

;
; General installation section
;

[iteraid]
AddReg=iteraid.AddReg
CopyFiles=iteraid.Miniport
Reboot

[iteraid.AddReg]

;
; File sections
;

[iteraid.Miniport]
iteraid.sys

;
; Service Installation
;

[iteraid.Services]
AddService = iteraid, 0x00000002 , iteraid_Service_Inst, iteraid_EventLog_Inst

[iteraid_Service_Inst]
DisplayName    = %iteraid.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_SYSTEM_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\iteraid.sys
AddReg         = pnpsafe_pci_addreg

[iteraid_EventLog_Inst]
AddReg = iteraid_EventLog_AddReg

[iteraid_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\iteraid.sys"
HKR,,TypesSupported,0x00010001,7

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

;
; Source file information
;

[SourceDisksNames.x86]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iteraid.sys = 1,,

[Strings]
ITE.DeviceDesc0 = "ITE IT8212 ATA RAID Controller"
DiskId1 = "ITE IT8212 ATA RAID Controller Driver Diskette"
ITE = "Integrated Technology Express, Inc."
iteraid.SvcDesc="ITERAID_Service_Install"