;========================================== 
; This is a Setup information file for monitors  with ICM  file; 
; Copyright 2024 AsRock  Electronics Co.
;==========================================
 
[version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%ASROCK%
CatalogFile=PG34QRT3A.cat   
DriverVer=06/25/2024,1.0.0.0

[ControlFlags]

ExcludeFromSelect.nt=Monitor\ASRAAA3
ExcludeFromSelect.nt=Monitor\ASRAAA3

[DestinationDirs]
DefaultDestDir=11
PG34QRT3A_HDMI.CopyFiles=23
PG34QRT3A_DP.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,

[SourceDisksFiles]
PG34QRT3A.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%ASROCK%=ASROCK,NTx86, NTamd64

[ASROCK]
%PG34QRT3A_HDMI%=PG34QRT3A_HDMI.Install, Monitor\ASRAAA3
%PG34QRT3A_DP%=PG34QRT3A_DP.Install, Monitor\ASRAAA3

[ASROCK.NTx86]
%PG34QRT3A_HDMI%=PG34QRT3A_HDMI.Install, Monitor\ASRAAA3
%PG34QRT3A_DP%=PG34QRT3A_DP.Install, Monitor\ASRAAA3


[ASROCK.NTamd64]
%PG34QRT3A_HDMI%=PG34QRT3A_HDMI.Install, Monitor\ASRAAA3
%PG34QRT3A_DP%=PG34QRT3A_DP.Install, Monitor\ASRAAA3

[PG34QRT3A_HDMI.Install]
DelReg=DEL_CURRENT_REG
AddReg=PG34QRT3A_HDMI.AddReg
Copyfiles=PG34QRT3A_HDMI.CopyFiles

[PG34QRT3A_DP.Install]
DelReg=DEL_CURRENT_REG
AddReg=PG34QRT3A_DP.AddReg
Copyfiles=PG34QRT3A_DP.CopyFiles


[PG34QRT3A_HDMI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[PG34QRT3A_DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install



[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile
HKR,,ICMProfileAC

; This sample installs both profiles to the advanced color (AC) profile association list.
; The presence of at least one valid ICC profile in the AC association list
; will enable WCG for the display.

[PG34QRT3A_HDMI.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30.0-160.0,48.0-120.0,-,+"
HKR,,MaxResolution,,"3440,1440"
HKR,,DPMS,,1
HKR,,ICMProfileAC,0,"PG34QRT3A.icm"
HKR,,DisplayHdrLevel, %REG_MULTI_SZ_APPEND%, 0D710BC2-6368-4EB2-A829-CBBD45CE3BD2

[PG34QRT3A_DP.AddReg]
HKR,"MODES\3440,1440",Mode1,,"275.0-275.0,48.0-180.0,-,+"
HKR,,MaxResolution,,"3440,1440"
HKR,,DPMS,,1
HKR,,ICMProfileAC,0,"PG34QRT3A.icm"
HKR,,DisplayHdrLevel, %REG_MULTI_SZ_APPEND%, 0D710BC2-6368-4EB2-A829-CBBD45CE3BD2, AE040E1F-51EC-4CAC-8501-E611C3C29CFE


[PG34QRT3A_HDMI.CopyFiles]
PG34QRT3A.icm

[PG34QRT3A_DP.CopyFiles]
PG34QRT3A.icm



[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

ASROCK="ASROCK"
Diskname="ASROCK PG34QRT3A Monitor installation diskette"
REG_MULTI_SZ_APPEND=0x00010008

PG34QRT3A_HDMI="PG34QRT3A"
PG34QRT3A_DP="PG34QRT3A"