;=======================================================
; P2410_TS_CAM.inf Ver. 1.0 03/07/2021
;
; Monitor INF file for Fujitsu Display P2410 TS CAM FHD
;
; Copyright 2019 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FTS-Mfg%
CatalogFile = P2140_TS_CAM.cat
DriverVer   = 03/07/2021, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
P2410_TS_CAM.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
P2410_TS_CAM.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS0908
ExcludeFromSelect = Monitor\FUS0909
ExcludeFromSelect = Monitor\FUS090A

[Manufacturer]
%FTS-Mfg% = FTS-Mfg, NTx86, NTAMD64

[FTS-Mfg]
%P2410_TS_CAM.HDMI%   = P2410_TS_CAM.HDMI.Install, Monitor\FUS0908
%P2410_TS_CAM.DP%     = P2410_TS_CAM.DP.Install, Monitor\FUS0909
%P2410_TS_CAM.USB-C%  = P2410_TS_CAM.USB-C.Install, Monitor\FUS090A

[FTS-Mfg.NTx86]

%P2410_TS_CAM.HDMI%   = P2410_TS_CAM.HDMI.Install, Monitor\FUS0908
%P2410_TS_CAM.DP%     = P2410_TS_CAM.DP.Install, Monitor\FUS0909
%P2410_TS_CAM.USB-C%  = P2410_TS_CAM.USB-C.Install, Monitor\FUS090A

[FTS-Mfg.NTAMD64]

%P2410_TS_CAM.HDMI%   = P2410_TS_CAM.HDMI.Install, Monitor\FUS0908
%P2410_TS_CAM.DP%     = P2410_TS_CAM.DP.Install, Monitor\FUS0909
%P2410_TS_CAM.USB-C%  = P2410_TS_CAM.USB-C.Install, Monitor\FUS090A


[P2410_TS_CAM.HDMI.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P2410_TS_CAM.HDMI.AddReg, 1920x1080, DPMS
CopyFiles = P2410_TS_CAM.CopyFiles

[P2410_TS_CAM.DP.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P2410_TS_CAM.DP.AddReg, 1920x1080, DPMS
CopyFiles = P2410_TS_CAM.CopyFiles

[P2410_TS_CAM.USB-C.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P2410_TS_CAM.USB-C.AddReg, 1920x1080, DPMS
CopyFiles = P2410_TS_CAM.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[P2410_TS_CAM.HDMI.AddReg]
HKR,"MODES\1920,1080",Mode1,,"48-76,30-82,+,+"
HKR,,ICMProfile,0,"P2410_TS_CAM.icm"

[P2410_TS_CAM.DP.AddReg]
HKR,"MODES\1920,1080",Mode1,,"48-76,30-82,+,+"
HKR,,ICMProfile,0,"P2410_TS_CAM.icm"

[P2410_TS_CAM.USB-C.AddReg]
HKR,"MODES\1920,1080",Mode1,,"48-76,30-82,+,+"
HKR,,ICMProfile,0,"P2410_TS_CAM.icm"

[1920x1080]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[P2410_TS_CAM.CopyFiles]
P2410_TS_CAM.icm

[P2410_TS_CAM.HDMI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P2410_TS_CAM.DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P2410_TS_CAM.USB-C.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FTS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

P2410_TS_CAM.HDMI  = "Fujitsu P2410 TS CAM (HDMI)"
P2410_TS_CAM.DP    = "Fujitsu P2410 TS CAM (DP)"
P2410_TS_CAM.USB-C = "Fujitsu P2410 TS CAM (USB-C)"
