;-------------------------------------------------------------------------------
;
; Motorola USB Remote NDIS Driver (motrndis.inf)
;
; Copyright (c) 2010-2015 Motorola
;
;-------------------------------------------------------------------------------;                     

[Version]
Signature           = "$Windows NT$"
Class               = Net
ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider            = %Motorola%
DriverVer           = 11/08/2011, 1.0.5.0
CatalogFile         = motrndis.cat

[Manufacturer]
%Motorola%          = Motorola,ntx86.5.1,ntx86.6.0,ntamd64

; Not supporting Windows 2000 anymore
[Motorola]

; XP supported
[Motorola.ntx86.5.1]

; t qc
%Motrndis.DeviceDesc%	= RNDIS.NT.5.1, USB\VID_22B8&PID_2E19&MI_00
%Motrndis.DeviceDesc%	= RNDIS.NT.5.1, USB\VID_22B8&PID_2E1A&MI_00

; p qc
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_2DFC
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_2DFD&MI_00

; o4-1
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_431C
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_431D&MI_00
; o4-2
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_4338
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_4339&MI_00
; dq+
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_2DE9&MI_00
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_2DEB&MI_00

; et
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_7095&MI_00
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_7096&MI_00
; ev
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70B2&MI_00
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70B3&MI_00
; t o4
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_42FC
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_42FD&MI_00
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_4303&MI_00
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_4304&MI_00
; s o4
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_42DC
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_42DD&MI_00
; d nV
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70CC
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70CD&MI_00

; e
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70AE
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_70AF&MI_00
; o3
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_41E4
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_41E5&MI_00
; o/e
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_7091
%Motrndis.DeviceDesc%    = RNDIS.NT.5.1, USB\VID_22B8&PID_7092&MI_00

%Motrndis.DeviceDesc%    = MOTRNDISTEST.NT.5.1, USB\VID_22B8&PID_41EE&MI_08

; Vista and higher not needed
[Motorola.ntx86.6.0]

; x64 not needed 
[Motorola.ntamd64]

[ControlFlags]
ExcludeFromSelect=*

; Windows XP and later sections -----------------------------------

[RNDIS.NT.5.1]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
include         = netrndis.inf
needs           = Usb_Rndis.ndi

; no copyfiles - the files are already in place

[RNDIS.NT.5.1.Services]
include     = netrndis.inf
needs       = Usb_Rndis.ndi.Services


; Test sections -----------------------------------------------------
[MOTRNDISTEST.NT.5.1]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15;

[MOTRNDISTEST.NT.5.1.Services]
AddService = ,2    ;



[Strings]
Motorola              = "Motorola"
Motrndis.DeviceDesc   = "Motorola USB RNDIS Device"




